Debug:(toolbox.cpp:84, ) ToolBox Start.....
Debug:(:0, ) QObject::connect: No such signal LogWnd::close()
Debug:(:0, ) QObject::connect:  (sender name:   'LogWnd')
Debug:(:0, ) QObject::connect:  (receiver name: 'LogWnd')
Debug:(toolbox.cpp:2251, ) "//192.168.5.50/Tftp32/UrsaLink/Images_Test/Toolbox_PC/ToolBox/translations/ToolBox_zh_CN.qm"
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:202, ) m_loraReadIndex: 50921736 false false
Debug:(qunpbasic.cpp:1961, ) false "COM7" "COM7"
Debug:(qunpbasic.cpp:1969, ) "拒绝访问。" QSerialPort::PermissionError
Debug:(connectting.cpp:288, ) close serial port
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qnfcbasic.cpp:243, ) "" 0
Debug:(qnfcbasic.cpp:244, ) ## pktsize: 1158

Debug:(qnfcbasic.cpp:245, ) ## flash_size: 1024

Debug:(qnfcbasic.cpp:246, ) ############# d3fc93e9

Debug:(qnfcbasic.cpp:247, ) ############# d3fc93e9

Debug:(connectting.cpp:185, ) #####m_flashType: 1
Debug:(connectting.cpp:224, ) Device Connect Success
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpbasic.cpp:2190, ) pn--- 868M

Debug:(qunpbasic.cpp:2347, ) pn3--- 

Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 11 len 8
Debug:(connectting.cpp:257, ) product name pn:  "AM103-868M"
Debug:(connectting.cpp:288, ) close serial port
68M" "" "01.05" "1.1" 0 0
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpam103.cpp:689, ) pn--- 868M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "0000" "AM103-868M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 1724807519 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 1724807519 0 "2024-08-28 01:11:59" "01:11:59"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 0
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "32" "32"
Debug:(dealam103Thread.cpp:121, ) request type:3
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1426, ) [NFC发送数据:]  "4d3c2b1a785634120102030000000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcbasic.cpp:1469, ) recv_buf1 send_num=0  len=0

Debug:(dealam103Thread.cpp:1075, ) false 0
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) true "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpbasic.cpp:2190, ) pn--- 868M

Debug:(qnfcbasic.cpp:193, ) product... "AM103" "868M" "1.1" "01.05" 0
Debug:(qnfcbasic.cpp:197, ) "AM103" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# 55f6fcd1

Debug:(qnfcbasic.cpp:200, ) ############# 55f6fcd1

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpam103.cpp:689, ) pn--- 868M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "0000" "AM103-868M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 43210 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 43210 0 "1970-01-01 12:00:10" "12:00:10"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 0
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "32" "32"
Debug:(:0, ) QIODevice::write (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpbasic.cpp:2190, ) pn--- 868M

Debug:(qnfcbasic.cpp:193, ) product... "AM103" "868M" "1.1" "01.05" 0
Debug:(qnfcbasic.cpp:197, ) "AM103" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# 55f6fcd1

Debug:(qnfcbasic.cpp:200, ) ############# 55f6fcd1

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpam103.cpp:689, ) pn--- 868M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "0000" "AM103-868M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 43216 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 43216 0 "1970-01-01 12:00:16" "12:00:16"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 0
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "32" "32"
Debug:(dealam103Thread.cpp:121, ) request type:3
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1426, ) [NFC发送数据:]  "4d3c2b1a785634120102020000000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcbasic.cpp:1469, ) recv_buf1 send_num=0  len=0

Debug:(dealam103Thread.cpp:1075, ) true 0
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) true "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpbasic.cpp:2190, ) pn--- 868M

Debug:(qnfcbasic.cpp:193, ) product... "AM103" "868M" "1.1" "01.05" 0
Debug:(qnfcbasic.cpp:197, ) "AM103" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# 47b2bbd2

Debug:(qnfcbasic.cpp:200, ) ############# 47b2bbd2

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpam103.cpp:689, ) pn--- 868M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "0000" "AM103-868M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 43236 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 43236 0 "1970-01-01 12:00:36" "12:00:36"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 0
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "32" "32"
Debug:(:0, ) QIODevice::write (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(connectting.cpp:550, ) request type:0  isNfc:1
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 0 len 106
Debug:(connectting.cpp:781, ) chanMask: "0007" "0" "85"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 106 len 100
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 215 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 216 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 248 len 8
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 214 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 218 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 217 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 219 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 96 len 10
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 221 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 212 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 222 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 249 len 200
Debug:(connectting.cpp:889, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:890, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:891, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:892, ) group[0] mode:0  devaddr:0000 
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:202, ) m_loraReadIndex: -1 false false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:220, ) [Rx2 freq ] "869525000" "0" "2" "4"
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:804, ) "868100000" "868300000" "868500000" "0"
Debug:(dealam103Thread.cpp:121, ) request type:1
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 0
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "32" "32"
Debug:(connectting.cpp:550, ) request type:0  isNfc:1
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 0 len 106
Debug:(connectting.cpp:781, ) chanMask: "0007" "0" "85"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 106 len 100
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 215 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 216 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 248 len 8
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 214 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 218 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 217 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 219 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 96 len 10
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 221 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 212 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 222 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 249 len 200
Debug:(connectting.cpp:889, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:890, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:891, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:892, ) group[0] mode:0  devaddr:0000 
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:202, ) m_loraReadIndex: -1 false false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:220, ) [Rx2 freq ] "869525000" "0" "2" "4"
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:804, ) "868100000" "868300000" "868500000" "0"
Debug:(connectting.cpp:550, ) request type:0  isNfc:1
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 0 len 106
Debug:(connectting.cpp:781, ) chanMask: "0007" "0" "85"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 106 len 100
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 215 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 216 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 248 len 8
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 214 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 218 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 217 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 219 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 96 len 10
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 221 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 212 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 222 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 249 len 200
Debug:(connectting.cpp:889, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:890, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:891, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:892, ) group[0] mode:0  devaddr:0000 
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:202, ) m_loraReadIndex: -1 false false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:220, ) [Rx2 freq ] "869525000" "0" "2" "4"
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:804, ) "868100000" "868300000" "868500000" "0"
Debug:(dealam103Thread.cpp:121, ) request type:1
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 0
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "32" "32"
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpbasic.cpp:2190, ) pn--- 868M

Debug:(qnfcbasic.cpp:193, ) product... "AM103" "868M" "1.1" "01.05" 0
Debug:(qnfcbasic.cpp:197, ) "AM103" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# 54248227

Debug:(qnfcbasic.cpp:200, ) ############# 54248227

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpam103.cpp:689, ) pn--- 868M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "0000" "AM103-868M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 43939 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 43939 0 "1970-01-01 12:12:19" "12:12:19"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 0
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "32" "32"
Debug:(connectting.cpp:550, ) request type:0  isNfc:1
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 0 len 106
Debug:(connectting.cpp:781, ) chanMask: "0007" "0" "85"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 106 len 100
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 215 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 216 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 248 len 8
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 214 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 218 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 217 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 219 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 96 len 10
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 221 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 212 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 222 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 249 len 200
Debug:(connectting.cpp:889, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:890, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:891, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:892, ) group[0] mode:0  devaddr:0000 
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:202, ) m_loraReadIndex: -1 false false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:220, ) [Rx2 freq ] "869525000" "0" "2" "4"
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:804, ) "868100000" "868300000" "868500000" "0"
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:202, ) m_loraReadIndex: -1 false false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:220, ) [Rx2 freq ] "869525000" "0" "2" "4"
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:804, ) "868100000" "868300000" "868500000" "0"
Debug:(toolbox.cpp:2251, ) "//192.168.5.50/Tftp32/UrsaLink/Images_Test/Toolbox_PC/ToolBox/translations/ToolBox_zh_CN.qm"
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:202, ) m_loraReadIndex: -1 false false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:220, ) [Rx2 freq ] "869525000" "0" "2" "4"
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:804, ) "868100000" "868300000" "868500000" "0"
Debug:(basicmethod.cpp:66, ) lora Rx2 Freq Range max min value region 870000000 863000000 869525000 4
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpbasic.cpp:2190, ) pn--- 868M

Debug:(qnfcbasic.cpp:193, ) product... "AM103" "868M" "1.1" "01.05" 0
Debug:(qnfcbasic.cpp:197, ) "AM103" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# 0e7624e8

Debug:(qnfcbasic.cpp:200, ) ############# 0e7624e8

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpam103.cpp:689, ) pn--- 868M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "0000" "AM103-868M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 44266 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 44266 0 "1970-01-01 12:17:46" "12:17:46"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 0
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "32" "32"
Debug:(dealam103Thread.cpp:121, ) request type:3
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1426, ) [NFC发送数据:]  "4d3c2b1a785634120102030000000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcbasic.cpp:1469, ) recv_buf1 send_num=0  len=0

Debug:(dealam103Thread.cpp:1075, ) false 0
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) true "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpbasic.cpp:2190, ) pn--- 868M

Debug:(qnfcbasic.cpp:193, ) product... "AM103" "868M" "1.1" "01.05" 0
Debug:(qnfcbasic.cpp:197, ) "AM103" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# 55f6fcd1

Debug:(qnfcbasic.cpp:200, ) ############# 55f6fcd1

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpam103.cpp:689, ) pn--- 868M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "0000" "AM103-868M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 43210 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 43210 0 "1970-01-01 12:00:10" "12:00:10"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 0
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "32" "32"
Debug:(:0, ) QIODevice::write (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(dealam103Thread.cpp:121, ) request type:3
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1426, ) [NFC发送数据:]  "4d3c2b1a785634120102020000000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcbasic.cpp:1469, ) recv_buf1 send_num=0  len=0

Debug:(dealam103Thread.cpp:1075, ) true 0
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) true "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpbasic.cpp:2190, ) pn--- 868M

Debug:(qnfcbasic.cpp:193, ) product... "AM103" "868M" "1.1" "01.05" 0
Debug:(qnfcbasic.cpp:197, ) "AM103" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# 47b2bbd2

Debug:(qnfcbasic.cpp:200, ) ############# 47b2bbd2

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpam103.cpp:689, ) pn--- 868M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "0000" "AM103-868M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 43230 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 43230 0 "1970-01-01 12:00:30" "12:00:30"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 0
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "32" "32"
Debug:(:0, ) QIODevice::write (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(connectting.cpp:550, ) request type:0  isNfc:1
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 0 len 106
Debug:(connectting.cpp:781, ) chanMask: "0007" "0" "85"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 106 len 100
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 215 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 216 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 248 len 8
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 214 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 218 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 217 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 219 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 96 len 10
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 221 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 212 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 222 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 249 len 200
Debug:(connectting.cpp:889, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:890, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:891, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:892, ) group[0] mode:0  devaddr:0000 
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:202, ) m_loraReadIndex: -1 false true
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:220, ) [Rx2 freq ] "869525000" "0" "2" "4"
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:804, ) "868100000" "868300000" "868500000" "0"
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpbasic.cpp:2190, ) pn--- 868M

Debug:(qnfcbasic.cpp:193, ) product... "AM103" "868M" "1.1" "01.05" 0
Debug:(qnfcbasic.cpp:197, ) "AM103" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# b4843555

Debug:(qnfcbasic.cpp:200, ) ############# b4843555

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpam103.cpp:689, ) pn--- 868M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "0000" "AM103-868M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 43298 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 43298 0 "1970-01-01 12:01:38" "12:01:38"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 0
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "32" "32"
Debug:(dealam103Thread.cpp:121, ) request type:3
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1426, ) [NFC发送数据:]  "4d3c2b1a785634120102030000000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcbasic.cpp:1469, ) recv_buf1 send_num=0  len=0

Debug:(dealam103Thread.cpp:1075, ) false 0
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) true "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpbasic.cpp:2190, ) pn--- 868M

Debug:(qnfcbasic.cpp:193, ) product... "AM103" "868M" "1.1" "01.05" 0
Debug:(qnfcbasic.cpp:197, ) "AM103" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# 55f6fcd1

Debug:(qnfcbasic.cpp:200, ) ############# 55f6fcd1

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpam103.cpp:689, ) pn--- 868M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "0000" "AM103-868M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 43210 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 43210 0 "1970-01-01 12:00:10" "12:00:10"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 0
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "32" "32"
Debug:(:0, ) QIODevice::write (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpbasic.cpp:2190, ) pn--- 868M

Debug:(qnfcbasic.cpp:193, ) product... "AM103" "868M" "1.1" "01.05" 0
Debug:(qnfcbasic.cpp:197, ) "AM103" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# 55f6fcd1

Debug:(qnfcbasic.cpp:200, ) ############# 55f6fcd1

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpam103.cpp:689, ) pn--- 868M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "0000" "AM103-868M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 43216 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 43216 0 "1970-01-01 12:00:16" "12:00:16"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 0
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "32" "32"
Debug:(dealam103Thread.cpp:121, ) request type:3
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1426, ) [NFC发送数据:]  "4d3c2b1a785634120102020000000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcbasic.cpp:1469, ) recv_buf1 send_num=0  len=0

Debug:(dealam103Thread.cpp:1075, ) true 0
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) true "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpbasic.cpp:2190, ) pn--- 868M

Debug:(qnfcbasic.cpp:193, ) product... "AM103" "868M" "1.1" "01.05" 0
Debug:(qnfcbasic.cpp:197, ) "AM103" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# 47b2bbd2

Debug:(qnfcbasic.cpp:200, ) ############# 47b2bbd2

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpam103.cpp:689, ) pn--- 868M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "0000" "AM103-868M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 43235 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 43235 0 "1970-01-01 12:00:35" "12:00:35"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 0
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "32" "32"
Debug:(:0, ) QIODevice::write (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpbasic.cpp:2190, ) pn--- 868M

Debug:(qnfcbasic.cpp:193, ) product... "AM103" "868M" "1.1" "01.05" 0
Debug:(qnfcbasic.cpp:197, ) "AM103" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# 30b67d87

Debug:(qnfcbasic.cpp:200, ) ############# 30b67d87

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpam103.cpp:689, ) pn--- 868M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "0000" "AM103-868M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 43708 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 43708 0 "1970-01-01 12:08:28" "12:08:28"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 0
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "32" "32"
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpbasic.cpp:2190, ) pn--- 868M

Debug:(qnfcbasic.cpp:193, ) product... "AM103" "868M" "1.1" "01.05" 0
Debug:(qnfcbasic.cpp:197, ) "AM103" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# 281196e2

Debug:(qnfcbasic.cpp:200, ) ############# 281196e2

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpam103.cpp:689, ) pn--- 868M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "0000" "AM103-868M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 43913 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 43913 0 "1970-01-01 12:11:53" "12:11:53"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 0
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "32" "32"
Debug:(connectting.cpp:550, ) request type:0  isNfc:1
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 0 len 106
Debug:(connectting.cpp:781, ) chanMask: "0007" "0" "85"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 106 len 100
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 215 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 216 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 248 len 8
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 214 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 218 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 217 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 219 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 96 len 10
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 221 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 212 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 222 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 249 len 200
Debug:(connectting.cpp:889, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:890, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:891, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:892, ) group[0] mode:0  devaddr:0000 
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:202, ) m_loraReadIndex: -1 false true
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:220, ) [Rx2 freq ] "869525000" "0" "2" "4"
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:804, ) "868100000" "868300000" "868500000" "0"
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qunpbasic.cpp:1969, ) "拒绝访问。" QSerialPort::PermissionError
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpbasic.cpp:2190, ) pn--- 868M

Debug:(qnfcbasic.cpp:193, ) product... "AM103" "868M" "1.1" "01.05" 0
Debug:(qnfcbasic.cpp:197, ) "AM103" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# f48b8ea2

Debug:(qnfcbasic.cpp:200, ) ############# f48b8ea2

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpam103.cpp:689, ) pn--- 868M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "0000" "AM103-868M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 43925 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 43925 0 "1970-01-01 12:12:05" "12:12:05"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 0
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "32" "32"
Debug:(connectting.cpp:550, ) request type:0  isNfc:1
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 0 len 106
Debug:(connectting.cpp:781, ) chanMask: "0007" "0" "85"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 106 len 100
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 215 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 216 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 248 len 8
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 214 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 218 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 217 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 219 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 96 len 10
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 221 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 212 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 222 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 249 len 200
Debug:(connectting.cpp:889, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:890, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:891, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:892, ) group[0] mode:0  devaddr:0000 
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:202, ) m_loraReadIndex: -1 false true
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:220, ) [Rx2 freq ] "869525000" "0" "2" "4"
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:804, ) "868100000" "868300000" "868500000" "0"
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpbasic.cpp:2190, ) pn--- 868M

Debug:(qnfcbasic.cpp:193, ) product... "AM103" "868M" "1.1" "01.05" 0
Debug:(qnfcbasic.cpp:197, ) "AM103" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# eb6a867c

Debug:(qnfcbasic.cpp:200, ) ############# eb6a867c

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpam103.cpp:689, ) pn--- 868M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "0000" "AM103-868M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 44171 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 44171 0 "1970-01-01 12:16:11" "12:16:11"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 0
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "32" "32"
Debug:(dealam103Thread.cpp:121, ) request type:3
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1426, ) [NFC发送数据:]  "4d3c2b1a785634120102030000000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcbasic.cpp:1469, ) recv_buf1 send_num=0  len=0

Debug:(dealam103Thread.cpp:1075, ) false 0
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) true "COM9" "COM9"
Debug:(qnfcbasic.cpp:949, ) [pn532_recv_data fail:] 4294967295
Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... AM103 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "AM103"
Debug:(qunpam103.cpp:689, ) pn--- 868M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "0000" "AM103-868M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 44171 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 44171 0 "1970-01-01 12:16:11" "12:16:11"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 0
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "32" "32"
Debug:(:0, ) QIODevice::write (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... EM500 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "EM500"
Debug:(qunpbasic.cpp:2190, ) pn--- CO2-470M

Debug:(qnfcbasic.cpp:193, ) product... "EM500" "CO2-470M" "2.0" "01.07" 0
Debug:(qnfcbasic.cpp:197, ) "EM500" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# c75ed9ae

Debug:(qnfcbasic.cpp:200, ) ############# c75ed9ae

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... EM500 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "EM500"
Debug:(qunpam103.cpp:689, ) pn--- CO2-470M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "470" "EM500-CO2-470M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 44 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 44 0 "1970-01-01 00:00:44" "00:00:44"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 1
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "0" "0"
Debug:(dealam103Thread.cpp:121, ) request type:3
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1426, ) [NFC发送数据:]  "4d3c2b1a785634120102020000000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcbasic.cpp:1469, ) recv_buf1 send_num=0  len=0

Debug:(dealam103Thread.cpp:1075, ) true 0
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) true "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... EM500 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "EM500"
Debug:(qunpbasic.cpp:2190, ) pn--- CO2-470M

Debug:(qnfcbasic.cpp:193, ) product... "EM500" "CO2-470M" "2.0" "01.07" 0
Debug:(qnfcbasic.cpp:197, ) "EM500" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# 27d04f6d

Debug:(qnfcbasic.cpp:200, ) ############# 27d04f6d

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... EM500 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "EM500"
Debug:(qunpam103.cpp:689, ) pn--- CO2-470M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "470" "EM500-CO2-470M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 64 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 64 0 "1970-01-01 00:01:04" "00:01:04"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 1
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "0" "0"
Debug:(:0, ) QIODevice::write (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(connectting.cpp:550, ) request type:0  isNfc:1
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 0 len 106
Debug:(connectting.cpp:781, ) chanMask: "0007" "0" "85"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 106 len 100
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 215 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 216 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 248 len 8
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 214 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 218 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 217 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 219 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 96 len 10
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 221 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 212 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 222 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 249 len 200
Debug:(connectting.cpp:889, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:890, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:891, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:892, ) group[0] mode:0  devaddr:0000 
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:202, ) m_loraReadIndex: -1 false true
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:220, ) [Rx2 freq ] "869525000" "0" "2" "4"
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:804, ) "868100000" "868300000" "868500000" "0"
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:202, ) m_loraReadIndex: -1 false true
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:220, ) [Rx2 freq ] "869525000" "0" "2" "4"
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:804, ) "868100000" "868300000" "868500000" "0"
Debug:(basicmethod.cpp:66, ) lora Rx2 Freq Range max min value region 870000000 863000000 869525000 4
Debug:(basicmethod.cpp:66, ) lora Rx2 Freq Range max min value region 870000000 863000000 869525000 4
Debug:(basicmethod.cpp:66, ) lora Rx2 Freq Range max min value region 870000000 863000000 869525000 4
Debug:(basicmethod.cpp:66, ) lora Rx2 Freq Range max min value region 870000000 863000000 869525000 4
Debug:(basicmethod.cpp:66, ) lora Rx2 Freq Range max min value region 870000000 863000000 869525000 4
Debug:(toolbox.cpp:2251, ) "//192.168.5.50/Tftp32/UrsaLink/Images_Test/Toolbox_PC/ToolBox/translations/ToolBox_zh_CN.qm"
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:202, ) m_loraReadIndex: -1 false true
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:220, ) [Rx2 freq ] "869525000" "0" "2" "4"
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:804, ) "868100000" "868300000" "868500000" "0"
Debug:(basicmethod.cpp:66, ) lora Rx2 Freq Range max min value region 870000000 863000000 869525000 4
Debug:(connectting.cpp:550, ) request type:2  isNfc:1
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(connectting.cpp:930, ) true false false
Debug:(connectting.cpp:1093, ) 1 true 0
Debug:(qnfcbasic.cpp:454, ) ######calulate_crc = a8a1729a

Debug:(qnfcbasic.cpp:1426, ) [NFC发送数据:]  "4d3c2b1a785634120102010605000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcbasic.cpp:1469, ) recv_buf1 send_num=20  len=1286

Debug:(qnfcbasic.cpp:1512, ) deal_with_nfc_ack err: "4d3c2b1a78563412010500000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000005500"
Debug:(connectting.cpp:471, ) connect nfc_set_flash: 1 "123456"  device_cmd: 1
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... EM500 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "EM500"
Debug:(qunpbasic.cpp:2190, ) pn--- CO2-470M

Debug:(qnfcbasic.cpp:193, ) product... "EM500" "CO2-470M" "2.0" "01.07" 0
Debug:(qnfcbasic.cpp:197, ) "EM500" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# 7acef15c

Debug:(qnfcbasic.cpp:200, ) ############# 7acef15c

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... EM500 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "EM500"
Debug:(qunpam103.cpp:689, ) pn--- CO2-470M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "470" "EM500-CO2-470M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 51 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 51 0 "1970-01-01 00:00:51" "00:00:51"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 1
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "0" "0"
Debug:(connectting.cpp:550, ) request type:0  isNfc:1
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 0 len 106
Debug:(connectting.cpp:781, ) chanMask: "0007" "0" "85"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 106 len 100
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 215 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 216 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 248 len 8
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 214 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 218 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 217 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 219 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 96 len 10
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 221 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 212 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 222 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 249 len 200
Debug:(connectting.cpp:889, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:890, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:891, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:892, ) group[0] mode:0  devaddr:0000 
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:202, ) m_loraReadIndex: -1 false false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:220, ) [Rx2 freq ] "869525000" "0" "2" "4"
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:804, ) "868100000" "868300000" "868500000" "0"
Debug:(basicmethod.cpp:66, ) lora Rx2 Freq Range max min value region 870000000 863000000 869525000 4
Debug:(connectting.cpp:550, ) request type:2  isNfc:1
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(connectting.cpp:930, ) true false false
Debug:(connectting.cpp:1093, ) 1 true 0
Debug:(qnfcbasic.cpp:454, ) ######calulate_crc = a8a1729a

Debug:(qnfcbasic.cpp:1426, ) [NFC发送数据:]  "4d3c2b1a785634120102010605000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcbasic.cpp:1469, ) recv_buf1 send_num=20  len=1286

Debug:(qnfcbasic.cpp:1512, ) deal_with_nfc_ack err: "4d3c2b1a78563412010500000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000005500"
Debug:(connectting.cpp:471, ) connect nfc_set_flash: 1 "123456"  device_cmd: 1
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... EM500 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "EM500"
Debug:(qunpbasic.cpp:2190, ) pn--- CO2-470M

Debug:(qnfcbasic.cpp:193, ) product... "EM500" "CO2-470M" "2.0" "01.07" 0
Debug:(qnfcbasic.cpp:197, ) "EM500" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# 7acef15c

Debug:(qnfcbasic.cpp:200, ) ############# 7acef15c

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... EM500 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "EM500"
Debug:(qunpam103.cpp:689, ) pn--- CO2-470M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "470" "EM500-CO2-470M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 122 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 122 0 "1970-01-01 00:02:02" "00:02:02"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 1
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "0" "0"
Debug:(connectting.cpp:550, ) request type:0  isNfc:1
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 0 len 106
Debug:(connectting.cpp:781, ) chanMask: "0007" "0" "85"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 106 len 100
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 215 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 216 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 248 len 8
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 214 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 218 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 217 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 219 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 96 len 10
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 221 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 212 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 222 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 249 len 200
Debug:(connectting.cpp:889, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:890, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:891, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:892, ) group[0] mode:0  devaddr:0000 
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:202, ) m_loraReadIndex: -1 false false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:220, ) [Rx2 freq ] "869525000" "0" "2" "4"
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:804, ) "868100000" "868300000" "868500000" "0"
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... EM500 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "EM500"
Debug:(qunpbasic.cpp:2190, ) pn--- CO2-470M

Debug:(qnfcbasic.cpp:193, ) product... "EM500" "CO2-470M" "2.0" "01.07" 0
Debug:(qnfcbasic.cpp:197, ) "EM500" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# 7acef15c

Debug:(qnfcbasic.cpp:200, ) ############# 7acef15c

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... EM500 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "EM500"
Debug:(qunpam103.cpp:689, ) pn--- CO2-470M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "470" "EM500-CO2-470M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 130 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 130 0 "1970-01-01 00:02:10" "00:02:10"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 1
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "0" "0"
Debug:(connectting.cpp:550, ) request type:0  isNfc:1
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 0 len 106
Debug:(connectting.cpp:781, ) chanMask: "0007" "0" "85"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 106 len 100
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 215 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 216 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 248 len 8
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 214 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 218 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 217 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 219 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 96 len 10
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 221 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 212 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 222 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 249 len 200
Debug:(connectting.cpp:889, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:890, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:891, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:892, ) group[0] mode:0  devaddr:0000 
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:202, ) m_loraReadIndex: -1 false false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:220, ) [Rx2 freq ] "869525000" "0" "2" "4"
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:804, ) "868100000" "868300000" "868500000" "0"
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... EM500 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "EM500"
Debug:(qunpbasic.cpp:2190, ) pn--- CO2-470M

Debug:(qnfcbasic.cpp:193, ) product... "EM500" "CO2-470M" "2.0" "01.07" 0
Debug:(qnfcbasic.cpp:197, ) "EM500" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# 7acef15c

Debug:(qnfcbasic.cpp:200, ) ############# 7acef15c

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... EM500 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "EM500"
Debug:(qunpam103.cpp:689, ) pn--- CO2-470M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "470" "EM500-CO2-470M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 170 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 170 0 "1970-01-01 00:02:50" "00:02:50"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 1
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "0" "0"
Debug:(connectting.cpp:550, ) request type:0  isNfc:1
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 0 len 106
Debug:(connectting.cpp:781, ) chanMask: "0007" "0" "85"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 106 len 100
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 215 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 216 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 248 len 8
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 214 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 218 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 217 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 219 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 96 len 10
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 221 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 212 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 222 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 249 len 200
Debug:(connectting.cpp:889, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:890, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:891, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:892, ) group[0] mode:0  devaddr:0000 
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:202, ) m_loraReadIndex: -1 false false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:220, ) [Rx2 freq ] "869525000" "0" "2" "4"
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:804, ) "868100000" "868300000" "868500000" "0"
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... EM500 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "EM500"
Debug:(qunpbasic.cpp:2190, ) pn--- CO2-470M

Debug:(qnfcbasic.cpp:193, ) product... "EM500" "CO2-470M" "2.0" "01.07" 0
Debug:(qnfcbasic.cpp:197, ) "EM500" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# 7acef15c

Debug:(qnfcbasic.cpp:200, ) ############# 7acef15c

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... EM500 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "EM500"
Debug:(qunpam103.cpp:689, ) pn--- CO2-470M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "470" "EM500-CO2-470M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 200 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 200 0 "1970-01-01 00:03:20" "00:03:20"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 1
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "0" "0"
Debug:(connectting.cpp:550, ) request type:0  isNfc:1
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 0 len 106
Debug:(connectting.cpp:781, ) chanMask: "0007" "0" "85"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 106 len 100
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 215 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 216 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 248 len 8
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 214 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 218 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 217 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 219 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 96 len 10
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 221 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 212 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 222 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 249 len 200
Debug:(connectting.cpp:889, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:890, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:891, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:892, ) group[0] mode:0  devaddr:0000 
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:202, ) m_loraReadIndex: -1 false false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:220, ) [Rx2 freq ] "869525000" "0" "2" "4"
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:804, ) "868100000" "868300000" "868500000" "0"
Debug:(basicmethod.cpp:66, ) lora Rx2 Freq Range max min value region 870000000 863000000 869525000 4
Debug:(connectting.cpp:550, ) request type:2  isNfc:1
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(connectting.cpp:930, ) true false false
Debug:(connectting.cpp:1093, ) 1 true 0
Debug:(qnfcbasic.cpp:454, ) ######calulate_crc = a8a1729a

Debug:(qnfcbasic.cpp:1426, ) [NFC发送数据:]  "4d3c2b1a785634120102010605000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcbasic.cpp:1469, ) recv_buf1 send_num=20  len=1286

Debug:(qnfcbasic.cpp:1512, ) deal_with_nfc_ack err: "4d3c2b1a78563412010500000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000005500"
Debug:(connectting.cpp:471, ) connect nfc_set_flash: 1 "123456"  device_cmd: 1
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... EM500 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "EM500"
Debug:(qunpbasic.cpp:2190, ) pn--- CO2-470M

Debug:(qnfcbasic.cpp:193, ) product... "EM500" "CO2-470M" "2.0" "01.07" 0
Debug:(qnfcbasic.cpp:197, ) "EM500" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# 7acef15c

Debug:(qnfcbasic.cpp:200, ) ############# 7acef15c

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... EM500 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "EM500"
Debug:(qunpam103.cpp:689, ) pn--- CO2-470M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "470" "EM500-CO2-470M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 266 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 266 0 "1970-01-01 00:04:26" "00:04:26"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 1
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "0" "0"
Debug:(connectting.cpp:550, ) request type:0  isNfc:1
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 0 len 106
Debug:(connectting.cpp:781, ) chanMask: "0007" "0" "85"
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 106 len 100
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 215 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 216 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 248 len 8
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 214 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 218 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 217 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 219 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 96 len 10
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 221 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 212 len 1
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 222 len 2
Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 249 len 200
Debug:(connectting.cpp:889, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:890, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:891, ) group[0] mode:0  devaddr:0000 
Debug:(connectting.cpp:892, ) group[0] mode:0  devaddr:0000 
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:202, ) m_loraReadIndex: -1 false false
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:220, ) [Rx2 freq ] "869525000" "0" "2" "4"
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  ""
Debug:(lorawanpage.cpp:997, ) () ("") 0 1
Debug:(lorawanpage.cpp:1012, ) partList: ("")
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:565, ) region:  "4"
Debug:(lorawanpage.cpp:804, ) "8681000000" "8683000000" "8685000000" ""
Debug:(lorawanpage.cpp:804, ) "868100000" "868300000" "868500000" "0"
Debug:(am103maintenancepage.cpp:19, ) [导入导出槽函数] 3
Debug:(dealam103Thread.cpp:121, ) request type:3
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1426, ) [NFC发送数据:]  "4d3c2b1a785634120102030000000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcbasic.cpp:1469, ) recv_buf1 send_num=0  len=0

Debug:(dealam103Thread.cpp:1075, ) false 0
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) true "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... EM500 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "EM500"
Debug:(qunpbasic.cpp:2190, ) pn--- CO2-470M

Debug:(qnfcbasic.cpp:193, ) product... "EM500" "CO2-470M" "2.0" "01.07" 0
Debug:(qnfcbasic.cpp:197, ) "EM500" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# 9a40679f

Debug:(qnfcbasic.cpp:200, ) ############# 9a40679f

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... EM500 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "EM500"
Debug:(qunpam103.cpp:689, ) pn--- CO2-470M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "470" "EM500-CO2-470M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 293 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 293 0 "1970-01-01 00:04:53" "00:04:53"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 1
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "0" "0"
Debug:(:0, ) QIODevice::write (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(am103maintenancepage.cpp:19, ) [导入导出槽函数] 4
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... EM500 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "EM500"
Debug:(qunpbasic.cpp:2190, ) pn--- CO2-470M

Debug:(qnfcbasic.cpp:193, ) product... "EM500" "CO2-470M" "2.0" "01.07" 0
Debug:(qnfcbasic.cpp:197, ) "EM500" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# 9a40679f

Debug:(qnfcbasic.cpp:200, ) ############# 9a40679f

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... EM500 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "EM500"
Debug:(qunpam103.cpp:689, ) pn--- CO2-470M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "470" "EM500-CO2-470M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 301 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 301 0 "1970-01-01 00:05:01" "00:05:01"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 1
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "0" "0"
Debug:(am103maintenancepage.cpp:19, ) [导入导出槽函数] 3
Debug:(dealam103Thread.cpp:121, ) request type:3
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1426, ) [NFC发送数据:]  "4d3c2b1a785634120102020000000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcbasic.cpp:1469, ) recv_buf1 send_num=0  len=0

Debug:(dealam103Thread.cpp:1075, ) true 0
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) true "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... EM500 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "EM500"
Debug:(qunpbasic.cpp:2190, ) pn--- CO2-470M

Debug:(qnfcbasic.cpp:193, ) product... "EM500" "CO2-470M" "2.0" "01.07" 0
Debug:(qnfcbasic.cpp:197, ) "EM500" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# 7acef15c

Debug:(qnfcbasic.cpp:200, ) ############# 7acef15c

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... EM500 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "EM500"
Debug:(qunpam103.cpp:689, ) pn--- CO2-470M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "470" "EM500-CO2-470M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 326 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 326 0 "1970-01-01 00:05:26" "00:05:26"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 1
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "0" "0"
Debug:(:0, ) QIODevice::write (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(:0, ) QIODevice::read (QSerialPort): device not open
Debug:(dealam103Thread.cpp:121, ) request type:0
Debug:(qunpbasic.cpp:1961, ) false "COM9" "COM9"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1158 [ACK DATA] "4d3c2b1a785634120100860400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1158, recv_num = 19
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... EM500 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "EM500"
Debug:(qunpbasic.cpp:2190, ) pn--- CO2-470M

Debug:(qnfcbasic.cpp:193, ) product... "EM500" "CO2-470M" "2.0" "01.07" 0
Debug:(qnfcbasic.cpp:197, ) "EM500" 0
Debug:(qnfcbasic.cpp:198, ) ## imagesize: 1158

Debug:(qnfcbasic.cpp:199, ) ############# 7acef15c

Debug:(qnfcbasic.cpp:200, ) ############# 7acef15c

Debug:(qunpbasic.cpp:2212, ) oemName--- 

Debug:(qunpbasic.cpp:2234, ) oempn--- 

Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... EM500 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "EM500"
Debug:(qunpam103.cpp:689, ) pn--- CO2-470M

Debug:(qunpam103.cpp:107, ) PARAM_UNXX_AX_RX:  ""
Debug:(qunpam103.cpp:748, ) unp_get_product_axrx....:  ""
Debug:(dealam103Thread.cpp:345, ) "470" "EM500-CO2-470M"
Debug:(qunpam103.cpp:802, ) pn3--- 

Debug:(dealam103Thread.cpp:389, ) [读时间戳] 333 [时区:] 0
Debug:(dealam103Thread.cpp:391, ) 333 0 "1970-01-01 00:05:33" "00:05:33"
Debug:(qunpam103.cpp:248, ) 248 block 0|1|2 0 0 1
Debug:(dealam103Thread.cpp:487, ) get threshold : "0" "0" "0" "0" "0"
