Debug:(toolbox.cpp:84, ) ToolBox Start.....
Debug:(:0, ) QObject::connect: No such signal LogWnd::close()
Debug:(:0, ) QObject::connect:  (sender name:   'LogWnd')
Debug:(:0, ) QObject::connect:  (receiver name: 'LogWnd')
Debug:(toolbox.cpp:2251, ) "C:/Users/admin/Desktop/ToolBox/translations/ToolBox_zh_CN.qm"
Debug:(lorawanpage.cpp:329, ) [m_multicast]  false [单火] false [Class B] false
Debug:(lorawanpage.cpp:202, ) m_loraReadIndex: 51544840 false false
Debug:(qunpbasic.cpp:1961, ) false "COM12" "COM12"
Debug:(qnfcbasic.cpp:1199, ) [ACK LEN] 1926 [ACK DATA] "4d3c2b1a785634120100860700000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000055"
Debug:(qnfcbasic.cpp:1207, ) ===recv_len = 1926, recv_num = 31
Debug:(qnfcbasic.cpp:1223, ) [recv:]  " "
Debug:(qnfcbasic.cpp:243, ) "" 0
Debug:(qnfcbasic.cpp:244, ) ## pktsize: 1926

Debug:(qnfcbasic.cpp:245, ) ## flash_size: 1792

Debug:(qnfcbasic.cpp:246, ) ############# d69eb16c

Debug:(qnfcbasic.cpp:247, ) ############# d69eb16c

Debug:(connectting.cpp:185, ) #####m_flashType: 2
Debug:(connectting.cpp:224, ) Device Connect Success
Debug:(qunpbasic.cpp:2155, ) connecting unp_get_product_name... UC501 
Debug:(qunpbasic.cpp:2161, ) connectting... m_product  "UC501"
Debug:(qunpbasic.cpp:2190, ) pn--- -470M

Debug:(qunpbasic.cpp:2347, ) pn3--- 

Debug:(qunpbasic.cpp:846, ) read lorawan param:80 pos 11 len 8
Debug:(connectting.cpp:257, ) product name pn:  "UC501--470M"
Debug:(connectting.cpp:288, ) close serial port
Debug:(toolbox.cpp:404, ) product name: "UC501--470M" "" "01.06" "3.0" 0 470
Debug:(uc50xv3dealthread.cpp:20, ) Thread id: 0x5130
Debug:(uc50xv3dealthread.cpp:118, ) request type:0
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101050000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:156, ) "UC501" UC501 0
Debug:(qnfcuc50xv3.cpp:160, ) ## imagesize: 1926

Debug:(qnfcuc50xv3.cpp:161, ) ############# d69eb16c

Debug:(qnfcuc50xv3.cpp:162, ) ############# d69eb16c

Debug:(qunpuc50xv3.cpp:3940, ) oemName--- 

Debug:(qunpuc50xv3.cpp:3962, ) oempn--- 

Debug:(qunpuc50xv3.cpp:621, ) ===== -470M
Debug:(qunpuc50xv3.cpp:2115, ) pn--- 470M

Debug:(uc50xv3dealthread.cpp:393, ) "UC501-470M"
Debug:(qunpuc50xv3.cpp:631, ) ===device oem:0086

Debug:(qunpuc50xv3.cpp:2212, ) pn3--- 

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 11 len 8

Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 214 len 1

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 0 len 106

Debug:(uc50xv3dealthread.cpp:617, ) appPort0000: "85" 0 0
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(ucchannelv3Page.cpp:30, ) onAddActionCmdSlot... 1
Debug:(uc50xv3generalpage.cpp:1360, ) "UC501-470M" "3.0"
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3generalpage.cpp:1360, ) "UC501-470M" "3.0"
Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101060000000000000000000003020000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:192, ) 
Debug:(uc50xv3dealthread.cpp:1592, ) GPIO Counter Fetch : 2
Debug:(uc50xv3dealthread.cpp:1603, ) 
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101080000000000000000000002000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(uc50xv3dealthread.cpp:1629, ) "2" "1"
Debug:(uc50xv3generalpage.cpp:1360, ) "UC501-470M" "3.0"
Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101060000000000000000000003010000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:192, ) 
Debug:(uc50xv3dealthread.cpp:1592, ) GPIO Counter Fetch : 1
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101080000000000000000000001000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(uc50xv3dealthread.cpp:1629, ) "" "1"
Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101060000000000000000000003010000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:192, ) 
Debug:(uc50xv3dealthread.cpp:1592, ) GPIO Counter Fetch : 1
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101080000000000000000000001000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(uc50xv3dealthread.cpp:1629, ) "" "1"
Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101060000000000000000000003020000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:192, ) 
Debug:(uc50xv3dealthread.cpp:1592, ) GPIO Counter Fetch : 2
Debug:(uc50xv3dealthread.cpp:1603, ) 
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101080000000000000000000002000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(uc50xv3dealthread.cpp:1629, ) "4" "1"
Debug:(uc50xv3dealthread.cpp:118, ) request type:0
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101050000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:156, ) "UC501" UC501 0
Debug:(qnfcuc50xv3.cpp:160, ) ## imagesize: 1926

Debug:(qnfcuc50xv3.cpp:161, ) ############# 21139de3

Debug:(qnfcuc50xv3.cpp:162, ) ############# 21139de3

Debug:(qunpuc50xv3.cpp:3940, ) oemName--- 

Debug:(qunpuc50xv3.cpp:3962, ) oempn--- 

Debug:(qunpuc50xv3.cpp:621, ) ===== -470M
Debug:(qunpuc50xv3.cpp:2115, ) pn--- 470M

Debug:(uc50xv3dealthread.cpp:393, ) "UC501-470M"
Debug:(qunpuc50xv3.cpp:631, ) ===device oem:0086

Debug:(qunpuc50xv3.cpp:2212, ) pn3--- 

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 11 len 8

Debug:(uc50xv3dealthread.cpp:118, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:705, ) setType: "gpio"
Debug:(uc50xv3dealthread.cpp:773, ) countChange: false false
Debug:(uc50xv3dealthread.cpp:811, ) 1
Debug:(uc50xv3dealthread.cpp:823, ) 1
Debug:(uc50xv3dealthread.cpp:118, ) request type:9
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:217, ) ######calulate_crc = c6f5df5c

Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a785634120102010607000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=28  len=1798

Debug:(uc50xv3dealthread.cpp:343, ) nfc_set_flash: 0 0
Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101060000000000000000000003010000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:192, ) 
Debug:(uc50xv3dealthread.cpp:1592, ) GPIO Counter Fetch : 1
Debug:(uc50xv3dealthread.cpp:1608, ) 
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101080000000000000000000001000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(uc50xv3dealthread.cpp:1629, ) "24" "1"
Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101060000000000000000000003020000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:192, ) 
Debug:(uc50xv3dealthread.cpp:1592, ) GPIO Counter Fetch : 2
Debug:(uc50xv3dealthread.cpp:1603, ) 
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101080000000000000000000002000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(uc50xv3dealthread.cpp:1629, ) "4" "1"
Debug:(uc50xv3generalpage.cpp:1360, ) "UC501-470M" "3.0"
Debug:(uc50xv3dealthread.cpp:118, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:705, ) setType: "gpio"
Debug:(uc50xv3dealthread.cpp:773, ) countChange: false false
Debug:(uc50xv3dealthread.cpp:118, ) request type:9
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:217, ) ######calulate_crc = 7610c598

Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a785634120102010607000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(uc50xv3dealthread.cpp:343, ) nfc_set_flash: 1 0
Debug:(uc50xv3dealthread.cpp:118, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:705, ) setType: "gpio"
Debug:(uc50xv3dealthread.cpp:773, ) countChange: false false
Debug:(uc50xv3dealthread.cpp:118, ) request type:9
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:217, ) ######calulate_crc = 7610c598

Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a785634120102010607000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=28  len=1798

Debug:(uc50xv3dealthread.cpp:343, ) nfc_set_flash: 0 0
Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:402, ) 3 1
Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a7856341201020e0000000031323334353603010000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(uc50xv3dealthread.cpp:118, ) request type:0
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:118, ) request type:0
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101050000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:156, ) "UC501" UC501 0
Debug:(qnfcuc50xv3.cpp:160, ) ## imagesize: 1926

Debug:(qnfcuc50xv3.cpp:161, ) ############# 609959eb

Debug:(qnfcuc50xv3.cpp:162, ) ############# 609959eb

Debug:(qunpuc50xv3.cpp:3940, ) oemName--- 

Debug:(qunpuc50xv3.cpp:3962, ) oempn--- 

Debug:(qunpuc50xv3.cpp:621, ) ===== -470M
Debug:(qunpuc50xv3.cpp:2115, ) pn--- 470M

Debug:(uc50xv3dealthread.cpp:393, ) "UC501-470M"
Debug:(qunpuc50xv3.cpp:631, ) ===device oem:0086

Debug:(qunpuc50xv3.cpp:2212, ) pn3--- 

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 11 len 8

Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101060000000000000000000003010000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:192, ) 
Debug:(uc50xv3dealthread.cpp:1137, ) GPIO1 Fetch :
Debug:(uc50xv3dealthread.cpp:1149, ) "0"
Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a7856341201020f0000000031323334353601010000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=0  len=0

Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a7856341201020f0000000031323334353601000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=0  len=0

Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a7856341201020f0000000031323334353601010000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=0  len=0

Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a7856341201020f0000000031323334353601000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=0  len=0

Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a7856341201020f0000000031323334353601010000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=0  len=0

Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a7856341201020f0000000031323334353601000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=0  len=0

Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:402, ) 3 1
Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a7856341201020e0000000031323334353603010000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101060000000000000000000003010000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:192, ) 
Debug:(uc50xv3dealthread.cpp:1137, ) GPIO1 Fetch :
Debug:(uc50xv3dealthread.cpp:1149, ) "1"
Debug:(uc50xv3dealthread.cpp:118, ) request type:0
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101050000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:156, ) "UC501" UC501 0
Debug:(qnfcuc50xv3.cpp:160, ) ## imagesize: 1926

Debug:(qnfcuc50xv3.cpp:161, ) ############# bb11c6ca

Debug:(qnfcuc50xv3.cpp:162, ) ############# bb11c6ca

Debug:(qunpuc50xv3.cpp:3940, ) oemName--- 

Debug:(qunpuc50xv3.cpp:3962, ) oempn--- 

Debug:(qunpuc50xv3.cpp:621, ) ===== -470M
Debug:(qunpuc50xv3.cpp:2115, ) pn--- 470M

Debug:(uc50xv3dealthread.cpp:393, ) "UC501-470M"
Debug:(qunpuc50xv3.cpp:631, ) ===device oem:0086

Debug:(qunpuc50xv3.cpp:2212, ) pn3--- 

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 11 len 8

Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 214 len 1

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 0 len 106

Debug:(uc50xv3dealthread.cpp:617, ) appPort0000: "85" 0 0
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(ucchannelv3Page.cpp:30, ) onAddActionCmdSlot... 1
Debug:(uc50xv3generalpage.cpp:1360, ) "UC501-470M" "3.0"
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 214 len 1

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 0 len 106

Debug:(uc50xv3dealthread.cpp:617, ) appPort0000: "85" 0 0
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(ucchannelv3Page.cpp:30, ) onAddActionCmdSlot... 1
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(uc50xv3dealthread.cpp:118, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:118, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:118, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:118, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:705, ) setType: "serial"
Debug:(qunpuc50xv3.cpp:2913, ) 0
Debug:(qunpuc50xv3.cpp:1332, ) uartcfg.app.enable11 = 0

Debug:(qunpuc50xv3.cpp:1335, ) uartcfg.app.enable22 = 1

Debug:(uc50xv3dealthread.cpp:118, ) request type:9
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:217, ) ######calulate_crc = 007efada

Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a785634120102010607000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=28  len=1798

Debug:(uc50xv3dealthread.cpp:343, ) nfc_set_flash: 0 2
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 214 len 1

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 0 len 106

Debug:(uc50xv3dealthread.cpp:617, ) appPort0000: "85" 0 0
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(ucchannelv3Page.cpp:30, ) onAddActionCmdSlot... 1
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 214 len 1

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 0 len 106

Debug:(uc50xv3dealthread.cpp:617, ) appPort0000: "85" 0 0
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(ucchannelv3Page.cpp:30, ) onAddActionCmdSlot... 1
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(uc50xv3dealthread.cpp:118, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:705, ) setType: "serial"
Debug:(qunpuc50xv3.cpp:2913, ) 0
Debug:(qunpuc50xv3.cpp:1332, ) uartcfg.app.enable11 = 1

Debug:(qunpuc50xv3.cpp:1335, ) uartcfg.app.enable22 = 1

Debug:(uc50xv3dealthread.cpp:118, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:705, ) setType: "serial"
Debug:(qunpuc50xv3.cpp:2913, ) 0
Debug:(qunpuc50xv3.cpp:1332, ) uartcfg.app.enable11 = 1

Debug:(qunpuc50xv3.cpp:1335, ) uartcfg.app.enable22 = 1

Debug:(uc50xv3dealthread.cpp:118, ) request type:9
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:217, ) ######calulate_crc = 27893f1c

Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a785634120102010607000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=28  len=1798

Debug:(uc50xv3dealthread.cpp:343, ) nfc_set_flash: 0 0
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 214 len 1

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 0 len 106

Debug:(uc50xv3dealthread.cpp:617, ) appPort0000: "85" 0 0
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(ucchannelv3Page.cpp:30, ) onAddActionCmdSlot... 1
Debug:(uc50xv3dealthread.cpp:118, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:705, ) setType: "serial"
Debug:(qunpuc50xv3.cpp:2913, ) 0
Debug:(qunpuc50xv3.cpp:1332, ) uartcfg.app.enable11 = 1

Debug:(qunpuc50xv3.cpp:1335, ) uartcfg.app.enable22 = 1

Debug:(uc50xv3dealthread.cpp:118, ) request type:0
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101050000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:156, ) "UC501" UC501 0
Debug:(qnfcuc50xv3.cpp:160, ) ## imagesize: 1926

Debug:(qnfcuc50xv3.cpp:161, ) ############# 6d421bf4

Debug:(qnfcuc50xv3.cpp:162, ) ############# 6d421bf4

Debug:(qunpuc50xv3.cpp:3940, ) oemName--- 

Debug:(qunpuc50xv3.cpp:3962, ) oempn--- 

Debug:(qunpuc50xv3.cpp:621, ) ===== -470M
Debug:(qunpuc50xv3.cpp:2115, ) pn--- 470M

Debug:(uc50xv3dealthread.cpp:393, ) "UC501-470M"
Debug:(qunpuc50xv3.cpp:631, ) ===device oem:0086

Debug:(qunpuc50xv3.cpp:2212, ) pn3--- 

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 11 len 8

Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 214 len 1

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 0 len 106

Debug:(uc50xv3dealthread.cpp:617, ) appPort0000: "85" 0 0
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(ucchannelv3Page.cpp:30, ) onAddActionCmdSlot... 1
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3generalpage.cpp:1360, ) "UC501-470M" "3.0"
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 214 len 1

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 0 len 106

Debug:(uc50xv3dealthread.cpp:617, ) appPort0000: "85" 0 0
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(ucchannelv3Page.cpp:30, ) onAddActionCmdSlot... 1
Debug:(uc50xv3dealthread.cpp:118, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:705, ) setType: "serial"
Debug:(qunpuc50xv3.cpp:2913, ) 0
Debug:(qunpuc50xv3.cpp:1332, ) uartcfg.app.enable11 = 1

Debug:(qunpuc50xv3.cpp:1335, ) uartcfg.app.enable22 = 1

Debug:(uc50xv3dealthread.cpp:118, ) request type:9
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:217, ) ######calulate_crc = ea3d6eb0

Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a785634120102010607000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=28  len=1798

Debug:(uc50xv3dealthread.cpp:343, ) nfc_set_flash: 0 0
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 214 len 1

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 0 len 106

Debug:(uc50xv3dealthread.cpp:617, ) appPort0000: "85" 0 0
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(ucchannelv3Page.cpp:30, ) onAddActionCmdSlot... 1
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(uc50xv3dealthread.cpp:118, ) request type:0
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101050000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:156, ) "UC501" UC501 0
Debug:(qnfcuc50xv3.cpp:160, ) ## imagesize: 1926

Debug:(qnfcuc50xv3.cpp:161, ) ############# c4901362

Debug:(qnfcuc50xv3.cpp:162, ) ############# c4901362

Debug:(qunpuc50xv3.cpp:3940, ) oemName--- 

Debug:(qunpuc50xv3.cpp:3962, ) oempn--- 

Debug:(qunpuc50xv3.cpp:621, ) ===== -470M
Debug:(qunpuc50xv3.cpp:2115, ) pn--- 470M

Debug:(uc50xv3dealthread.cpp:393, ) "UC501-470M"
Debug:(qunpuc50xv3.cpp:631, ) ===device oem:0086

Debug:(qunpuc50xv3.cpp:2212, ) pn3--- 

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 11 len 8

Debug:(uc50xv3dealthread.cpp:118, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:705, ) setType: "serial"
Debug:(qunpuc50xv3.cpp:2913, ) 0
Debug:(qunpuc50xv3.cpp:1332, ) uartcfg.app.enable11 = 1

Debug:(qunpuc50xv3.cpp:1335, ) uartcfg.app.enable22 = 1

Debug:(uc50xv3dealthread.cpp:118, ) request type:9
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:217, ) ######calulate_crc = af92f414

Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a785634120102010607000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=28  len=1798

Debug:(uc50xv3dealthread.cpp:343, ) nfc_set_flash: 0 2
Debug:(uc50xv3generalpage.cpp:2203, ) onFetchCmdSlot  1 type: 22 sign: 0
Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:1345, ) 1 1 ""
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101060000000000000000000002010000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:192, ) 
Debug:(uc50xv3dealthread.cpp:1455, ) 7 19 122 2
Debug:(uc50xv3generalpage.cpp:486, ) values: "122,"
Debug:(uc50xv3generalpage.cpp:494, ) "0" 1 "1" "0" 0
Debug:(uc50xv3generalpage.cpp:547, ) "0" 1 "1" "0" 0
Debug:(uc50xv3dealthread.cpp:118, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:705, ) setType: "serial"
Debug:(qunpuc50xv3.cpp:2913, ) 0
Debug:(qunpuc50xv3.cpp:1332, ) uartcfg.app.enable11 = 1

Debug:(qunpuc50xv3.cpp:1335, ) uartcfg.app.enable22 = 1

Debug:(uc50xv3dealthread.cpp:118, ) request type:9
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:217, ) ######calulate_crc = 71df7e9c

Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a785634120102010607000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=28  len=1798

Debug:(uc50xv3dealthread.cpp:343, ) nfc_set_flash: 0 0
Debug:(uc50xv3dealthread.cpp:118, ) request type:0
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101050000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:156, ) "UC501" UC501 0
Debug:(qnfcuc50xv3.cpp:160, ) ## imagesize: 1926

Debug:(qnfcuc50xv3.cpp:161, ) ############# bdfbd003

Debug:(qnfcuc50xv3.cpp:162, ) ############# bdfbd003

Debug:(qunpuc50xv3.cpp:3940, ) oemName--- 

Debug:(qunpuc50xv3.cpp:3962, ) oempn--- 

Debug:(qunpuc50xv3.cpp:621, ) ===== -470M
Debug:(qunpuc50xv3.cpp:2115, ) pn--- 470M

Debug:(uc50xv3dealthread.cpp:393, ) "UC501-470M"
Debug:(qunpuc50xv3.cpp:631, ) ===device oem:0086

Debug:(qunpuc50xv3.cpp:2212, ) pn3--- 

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 11 len 8

Debug:(uc50xv3dealthread.cpp:118, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:705, ) setType: "serial"
Debug:(qunpuc50xv3.cpp:2913, ) 0
Debug:(qunpuc50xv3.cpp:1332, ) uartcfg.app.enable11 = 1

Debug:(qunpuc50xv3.cpp:1335, ) uartcfg.app.enable22 = 1

Debug:(uc50xv3dealthread.cpp:118, ) request type:9
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:217, ) ######calulate_crc = ab830823

Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a785634120102010607000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=28  len=1798

Debug:(uc50xv3dealthread.cpp:343, ) nfc_set_flash: 0 0
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3generalpage.cpp:1360, ) "UC501-470M" "3.0"
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3generalpage.cpp:1360, ) "UC501-470M" "3.0"
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 214 len 1

Debug:(uc50xv3dealthread.cpp:591, ) Channel已使能： "UC501" 1 0
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 0 len 106

Debug:(uc50xv3dealthread.cpp:617, ) appPort0000: "85" 0 0
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(ucchannelv3Page.cpp:30, ) onAddActionCmdSlot... 1
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3generalpage.cpp:1360, ) "UC501-470M" "3.0"
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 214 len 1

Debug:(uc50xv3dealthread.cpp:591, ) Channel已使能： "UC501" 1 0
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 0 len 106

Debug:(uc50xv3dealthread.cpp:617, ) appPort0000: "85" 0 0
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(ucchannelv3Page.cpp:30, ) onAddActionCmdSlot... 1
Debug:(uc50xv3dealthread.cpp:118, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:705, ) setType: "serial"
Debug:(qunpuc50xv3.cpp:2913, ) 0
Debug:(qunpuc50xv3.cpp:1332, ) uartcfg.app.enable11 = 1

Debug:(qunpuc50xv3.cpp:1335, ) uartcfg.app.enable22 = 1

Debug:(uc50xv3dealthread.cpp:118, ) request type:9
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:217, ) ######calulate_crc = e0818047

Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a785634120102010607000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=28  len=1798

Debug:(uc50xv3dealthread.cpp:343, ) nfc_set_flash: 0 0
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 214 len 1

Debug:(uc50xv3dealthread.cpp:591, ) Channel已使能： "UC501" 1 0
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 0 len 106

Debug:(uc50xv3dealthread.cpp:617, ) appPort0000: "85" 0 0
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(ucchannelv3Page.cpp:30, ) onAddActionCmdSlot... 1
Debug:(uc50xv3dealthread.cpp:118, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:705, ) setType: "serial"
Debug:(qunpuc50xv3.cpp:2913, ) 0
Debug:(qunpuc50xv3.cpp:1332, ) uartcfg.app.enable11 = 1

Debug:(qunpuc50xv3.cpp:1335, ) uartcfg.app.enable22 = 1

Debug:(uc50xv3dealthread.cpp:118, ) request type:9
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:217, ) ######calulate_crc = a8972a45

Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a785634120102010607000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=28  len=1798

Debug:(uc50xv3dealthread.cpp:343, ) nfc_set_flash: 0 0
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3generalpage.cpp:1360, ) "UC501-470M" "3.0"
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 214 len 1

Debug:(uc50xv3dealthread.cpp:591, ) Channel已使能： "UC501" 1 0
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 0 len 106

Debug:(uc50xv3dealthread.cpp:617, ) appPort0000: "85" 0 0
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(ucchannelv3Page.cpp:30, ) onAddActionCmdSlot... 1
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:118, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:118, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:705, ) setType: "ai"
Debug:(uc50xv3dealthread.cpp:118, ) request type:9
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:217, ) ######calulate_crc = 496104d8

Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a785634120102010607000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=28  len=1798

Debug:(uc50xv3dealthread.cpp:343, ) nfc_set_flash: 0 0
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 214 len 1

Debug:(uc50xv3dealthread.cpp:591, ) Channel已使能： "UC501" 1 0
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 0 len 106

Debug:(uc50xv3dealthread.cpp:617, ) appPort0000: "85" 0 0
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(ucchannelv3Page.cpp:30, ) onAddActionCmdSlot... 1
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:118, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:705, ) setType: "ai"
Debug:(uc50xv3dealthread.cpp:118, ) request type:9
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:217, ) ######calulate_crc = 51a169a8

Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a785634120102010607000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=28  len=1798

Debug:(uc50xv3dealthread.cpp:343, ) nfc_set_flash: 0 0
Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:402, ) 1 1
Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a7856341201020e0000000031323334353601010000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=0  len=0

Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101060000000000000000000001010000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:192, ) 
Debug:(uc50xv3dealthread.cpp:1266, ) AI1 Fetch :
Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:402, ) 1 1
Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a7856341201020e0000000031323334353601010000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=0  len=0

Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101060000000000000000000001010000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:192, ) 
Debug:(uc50xv3dealthread.cpp:1266, ) AI1 Fetch :
Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:402, ) 1 1
Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a7856341201020e0000000031323334353601010000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=0  len=0

Debug:(uc50xv3dealthread.cpp:118, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:705, ) setType: "ai"
Debug:(uc50xv3dealthread.cpp:118, ) request type:9
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:217, ) ######calulate_crc = 51a169a8

Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a785634120102010607000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=28  len=1798

Debug:(uc50xv3dealthread.cpp:343, ) nfc_set_flash: 0 0
Debug:(uc50xv3dealthread.cpp:118, ) request type:0
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101050000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:156, ) "UC501" UC501 0
Debug:(qnfcuc50xv3.cpp:160, ) ## imagesize: 1926

Debug:(qnfcuc50xv3.cpp:161, ) ############# bcb9b8fc

Debug:(qnfcuc50xv3.cpp:162, ) ############# bcb9b8fc

Debug:(qunpuc50xv3.cpp:3940, ) oemName--- 

Debug:(qunpuc50xv3.cpp:3962, ) oempn--- 

Debug:(qunpuc50xv3.cpp:621, ) ===== -470M
Debug:(qunpuc50xv3.cpp:2115, ) pn--- 470M

Debug:(uc50xv3dealthread.cpp:393, ) "UC501-470M"
Debug:(qunpuc50xv3.cpp:631, ) ===device oem:0086

Debug:(qunpuc50xv3.cpp:2212, ) pn3--- 

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 11 len 8

Debug:(uc50xv3dealthread.cpp:118, ) request type:0
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101050000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:156, ) "UC501" UC501 0
Debug:(qnfcuc50xv3.cpp:160, ) ## imagesize: 1926

Debug:(qnfcuc50xv3.cpp:161, ) ############# 3316a79e

Debug:(qnfcuc50xv3.cpp:162, ) ############# 3316a79e

Debug:(qunpuc50xv3.cpp:3940, ) oemName--- 

Debug:(qunpuc50xv3.cpp:3962, ) oempn--- 

Debug:(qunpuc50xv3.cpp:621, ) ===== -470M
Debug:(qunpuc50xv3.cpp:2115, ) pn--- 470M

Debug:(uc50xv3dealthread.cpp:393, ) "UC501-470M"
Debug:(qunpuc50xv3.cpp:631, ) ===device oem:0086

Debug:(qunpuc50xv3.cpp:2212, ) pn3--- 

Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 11 len 8

Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 214 len 1

Debug:(uc50xv3dealthread.cpp:591, ) Channel已使能： "UC501" 1 0
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 0 len 106

Debug:(uc50xv3dealthread.cpp:617, ) appPort0000: "85" 0 0
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(ucchannelv3Page.cpp:30, ) onAddActionCmdSlot... 1
Debug:(uc50xv3generalpage.cpp:1360, ) "UC501-470M" "3.0"
Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101060000000000000000000001010000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:192, ) 
Debug:(uc50xv3dealthread.cpp:1266, ) AI1 Fetch :
Debug:(uc50xv3dealthread.cpp:118, ) request type:8
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:705, ) setType: "ai"
Debug:(uc50xv3dealthread.cpp:118, ) request type:9
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:217, ) ######calulate_crc = 1e21e69f

Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a785634120102010607000031323334353600000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=28  len=1798

Debug:(uc50xv3dealthread.cpp:343, ) nfc_set_flash: 0 0
Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:402, ) 1 2
Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a7856341201020e0000000031323334353601020000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=0  len=0

Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101060000000000000000000001020000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:192, ) 
Debug:(uc50xv3dealthread.cpp:1313, ) AI2 Fetch :
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 214 len 1

Debug:(uc50xv3dealthread.cpp:591, ) Channel已使能： "UC501" 1 0
Debug:(qunpuc50xv3.cpp:895, ) read lorawan param:80 pos 0 len 106

Debug:(uc50xv3dealthread.cpp:617, ) appPort0000: "85" 0 0
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(uc50xv3generalpage.cpp:2422, ) 
Debug:(ucchannelv3Page.cpp:30, ) onAddActionCmdSlot... 1
Debug:(uc50xv3dealthread.cpp:118, ) request type:1
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(uc50xv3dealthread.cpp:118, ) request type:17
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a785634120101160000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(ucchannelv3Page.cpp:178, ) onAddSdiActionCmdSlot... 1
Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a7856341201011700000000000000000000013f2100000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(uc50xv3dealthread.cpp:1881, ) num: 1 "?!"
Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a785634120102230000000031323334353601364137210000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=0  len=0

Debug:(uc50xv3dealthread.cpp:1881, ) num: 1 "6A7!"
Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1147, ) [NFC发送数据:]  "4d3c2b1a7856341201020e000000003132333435360401374d213b374430213b0000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1154, ) 1500
Debug:(qnfcuc50xv3.cpp:1160, ) after send connect data

Debug:(qnfcuc50xv3.cpp:1166, ) after recv connect data

Debug:(qnfcuc50xv3.cpp:1190, ) recv_buf1 send_num=0  len=0

Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1027, ) [NFC发送数据:]  "4d3c2b1a7856341201011700000000000000000000013f2100000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(uc50xv3dealthread.cpp:1881, ) num: 1 "?!"
Debug:(uc50xv3dealthread.cpp:118, ) request type:11
Debug:(qunpuc50xv3.cpp:1998, ) false "COM12" "COM12"
Debug:(qnfcuc50xv3.cpp:1085, ) [NFC发送数据:]  "4d3c2b1a785634120101060000000000000000000004017265616400000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(qnfcuc50xv3.cpp:1106, ) ===recv_len = 37, recv_num = 1

Debug:(qnfcuc50xv3.cpp:1114, ) [recv:]  0 "01372b312e302b302b32372e340d0a00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000"
Debug:(uc50xv3dealthread.cpp:1769, ) fetch value: "7+1.0+0+27.4\r\n"
Debug:(uc50xv3generalpage.cpp:670, ) "0" 2 "1" "0" 0
